
**Example Materials Laboratory**

**Benson I, Room 306**

Shape, rectangle, square

Description automatically generated**Principal Investigator: John Doe**

**AUTHORIZED PERSONNEL ONLY**

**EMERGENCY CONTACT 911**

**NOTICE**

U*of*SC Police Department: (803) 777-4215

EH&S Main Office: (803) 777-5269

Fire Safety: (803) 413-9359

Chemical & Lab Safety: (803) 351-9874

Biological Safety: (803) 622-3737

Radiation Safety: (803) 960-0169

Columbia Facilities: (803) 777-9675

**For any concerns on lab hazard, call numbers above.**

**RESEARCH GROUP**

**PI:** John Doe (803)-555-5555

**Members:**

Jane Doe (803) 555-5554


John Dae

John Dei

**WEAR ALL APPROPRIATE PERSONAL PROTECTIVE EQUIPMENT**

****

**NOTICE**

********

**REVIEW LIST OF LABORATORY HAZARDS BEFORE ENTRY**

****

**AUTHORIZED MINORS ONLY**

**CONTACT EH&S**

**NO SHORTS**

**NO SANDALS**

**NO FOOD OR DRINK**

**HAZARDS in BENSON I, 306**

**Consult lab Safety Manuals and Chemical Hygiene Plan for list of specific hazards.**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  | | --- | | Fire Hazards | | https://www.osha.gov/dsg/hazcom/pictograms/image2.jpg  Flammable liquid  **(6 gal)** | | https://www.osha.gov/dsg/hazcom/pictograms/image6.jpg  Gases under pressure | |  | | |  | | --- | | Health Hazards | | https://www.osha.gov/dsg/hazcom/pictograms/image4.jpg  Acutely toxic: **chromium oxide, nickel sulfate hexahydrate, palladium chloride** | | https://www.osha.gov/dsg/hazcom/pictograms/image9.jpghttps://www.osha.gov/dsg/hazcom/pictograms/image5.jpg  Irritants  Skin corrosion/burns, Eye damage  Corrosive to metals | | https://www.osha.gov/dsg/hazcom/pictograms/image7.jpgA yellow triangle sign  Description automatically generated with low confidence  Carcinogens  Asphyxiant (replaces oxygen in breathable air) | |

|  |  |
| --- | --- |
| Physical and Other Hazards | |
| Icon  Description automatically generated  Hot surfaces: **furnaces, kiln, hot plates, soldering iron** | A yellow sign with a black arrow  Description automatically generated with low confidence  Electrocution: **power supplies and vacuum furnace** |
| Cut/Sharps: **razors, needles, saws, hand tools** | ISO Symbols Labels - Crush Hazard | Seton  Pinch/crush: **Instron uniaxial load frame** |

|  |
| --- |
| Radiation Hazards |
| NONE |

|  |
| --- |
| Biological Hazards |
| NONE |